## Room comfort is becoming smart

# SIEGENIA Comfort app: Control windows and ventilators as well as entrance and sliding doors via WLAN

"Smart" by name, smart by nature: The motorised drives and ventilation systems from SIEGENIA. With the SIEGENIA Comfort app, the smart versions of these can be conveniently operated in all functions via smartphone or tablet and this therefore offers users convenient operation and monitoring of all functions. In this way, fabricators can benefit by offering private home owners a completely new dimension of room comfort. Both connection with the Comfort app and integration in the home WLAN network are very simple and function as quickly and effortlessly as with a smartphone. And when your own network is unavailable (e. g. on building sites), all solutions can also be connected directly with your smartphone.

#### Move large objects easily

Great emphasis is placed on comfort functions in the SIEGENIA Comfort app. For example, all lift-slide drives not only allow automatic opening and locking of heavy elements weighing up to 400 kg, but they also combine this with freely determinable opening widths and timed ventilation functions. The partially concealed DRIVE axxent HSA smart hardware meets the highest design standards. The concealed lift drive gives the element an appealing, elegant aesthetic that is also supported by its high quality operating unit for manual control.

#### For fresh air fanatics

This is how fresh air enters the building: With the two wall-mounted ventilators, AEROVITAL ambience smart and AEROTUBE smart, property owners have all options of individual control for demand-based ventilation on hand. This means end users can have fresh indoor air provided either with a tap of their finger or automatically, with sensor control. In addition to the continuous air flow regulation and the free choice of operating mode, the scope of performance also comprises individual timer and automatic functions as well as simple networking with other ventilators, sensors or window drives.

#### Entrance doors: securely locked or invitingly open according to your wishes

Lock entrance doors or make them freely accessible as required with a tap of your finger? This is also possible with the SIEGENIA Comfort app and the GENIUS electromechanical multi-point lock. While the door is completely locked in night mode, it is possible to deactivate the locking part during the day via the app when used in highly frequented areas. As with an E-opener, the door is then held shut by the latch only. The "permanently open function", adjustable via the app, enables free access.

#### Window, open yourself

The convenient operation of turn-and-tilt windows and tilt skylights, which are difficult to reach, is also included in the scope of performance of the SIEGENIA Comfort app. Concealed and therefore unobtrusive, DRIVE axxent DK moves sash weights of up to 130 kg. Thanks to its "two-in-one" principle, the drive combines all operating functions, making even the handle used for turning the window open surplus to requirements. In order to achieve high-quality room comfort concepts, the smart version also enables networking with sensors and opens the window independently in case of bad air in combination with the SENSOAIR smart air quality sensor.

DRIVE axxent MH, which was specially developed by SIEGENIA for the secured night vent, TITAN vent secure, is an ace with regard to security. The combination of these two solutions has been successfully tested in accordance with RC2 and enables ventilation via the secured night vent even if you are not at home. The efficient duo is currently being presented as a study.

#### Captions

Image database: SIEGENIA

### Image I: SIE\_DRIVE\_axxent HSA smart\_operation via App.jpg

With the comfort app, lift-slide drives from SIEGENIA allow automatic opening and locking of elements weighing up to 400 kg as well as connecting this with freely determinable opening widths.

### Image II: SIE\_AERO\_AEROVITAL ambience\_image\_woman.jpg

The Comfort app enables end users to activate SIEGENIA smart wall-mounted ventilators with the tap of a finger. Continuous air flow regulation and networking with other ventilators, sensors or window drives is also possible.

### Image III: SIE\_DRIVE\_axxent DK smart\_SIEGENIA Comfort App.jpg

Operate windows conveniently: The Comfort app takes over the control of elements with motorised drives. When combined with the SENSOAIR air quality sensor, this also includes automatic tilt ventilation in the event of stale air.

|  |  |  |
| --- | --- | --- |
| Publisher  SIEGENIA GROUP  Marketing Communications  Industriestraße 1-3  D-57234 Wilnsdorf Germany  Phone: +49 271 3931-412  Fax: +49 271 3931-77412  E-mail: pr@siegenia.com  www.siegenia.com/en | Edited by / Contact  Kemper Kommunikation  Kirsten Kemper  Feuerwehrstr. 42  D-51588 Nuembrecht Germany Phone: +49 2293 909890  Fax: +49 2293 909891  E-mail: info@kemper-kommunikation.de  www.kemper-kommunikation.de | Text details  Pages: 2  Words: 559  Characters: 3,515 (with spaces)  Created: 2018-03-21 |
| Please send us a sample copy of any publication containing this text or these images. | | |