## Versatile, durable and space-saving: ECO SLIDE CO from SIEGENIA

# New sliding hardware variants for a wide range of profile systems

Space-saving in use, sturdy in operation with the production benefits of turn-and-tilt hardware: the PORTAL ECO SLIDE CO from SIEGENIA combines room comfort qualities for end users with efficiency benefits in production. The further development of the tried-and-tested ECO SLIDE sliding hardware offers end users an attractive combination of ease of use, intuitive operation, energy efficiency and, above all, design. Fabricators will be won over by the new solution, which is obtainable alternatively to the tried-and-tested ECO SLIDE for Profine Premislide, due to its suitability for a wide range of profile systems and its especially cost-effective production. ECO SLIDE CO enables the easy integration of sliding components in the central locking gear for this purpose.

#### Space-saving solution with intuitive ease of use

As a versatile and space-saving solution, ECO SLIDE CO adapts perfectly to every room as a sliding window or sliding door. In contrast to classical balcony doors, the hardware offers convenient access to the outside thanks to its reduced passage height of approximately 45 mm in sliding doors. It combines the ease of use of a sliding solution with the advantages of turn-and-tilt hardware. Its wraparound design with its reliable compression provides a cosy feeling of well-being and high energy efficiency. Thus the ECO SLIDE CO is ideally suitable even for colder regions.

Its high standard of ease of use, in particular, is one of the greatest strengths of the new sliding hardware. Simultaneously sturdy and smooth-running, it is really intuitive to operate and therefore resistant to mishandling. This is ensured by the maintenance-free bogie wheels and the high-quality TITAN central locking gear, which makes it the ideal solution in case of frequently changing users. ECO SLIDE CO is also impressive in terms of the room comfort topics security and elegance: it can be flexibly upgraded to RC2, with only a few components, to increase the burglar resistance. Moreover, the hardware is available on request with valuable design components for discreet integration of the strikers in a locking rail. This gives fabricators additional scope of action for the design of tailor-made customer solutions.

#### Cost-effective all-rounder for a wide range of profile systems

ECO SLIDE CO also proves its qualities in production. The sliding systems from Gealan (Smoovio) and Rehau (Synego Slide) will be available as part of the market launch; further profile systems are in the preparation phase. Hence, the all-rounder offers fabricators a wide variety in its product offering for the individual design of sliding elements. Cost saving and time saving in production is ensured by the wraparound and tried-and-tested TITAN central sash hardware, for example, which can be assembled and adjusted with the aid of only a few additional components and only one multifunctional rail for the frame. This guarantees lean, efficient workflow from the warehousing to the assembly.

#### Captions

Image database: SIEGENIA

*Image I: SIE\_PORTAL\_ECO SLIDE CO\_Interieur\_Bad\_Presse.jpg*

As a sliding window, ECO SLIDE CO from SIEGENIA saves valuable interior space and adapts perfectly to every room. The hardware combines room comfort qualities for end users with cost-effectiveness in the production.

### Image II: SIE\_PORTAL\_ECO SLIDE CO\_Interieur\_Apartment\_Presse.jpg

In contrast to classical balcony doors, ECO SLIDE CO offers convenient access to the outside thanks to its reduced passage height of approximately 45 mm in sliding doors.

### Image III: SIE\_PORTAL\_ECO SLIDE CO\_Detail\_durchgehende\_Schließleiste.jpg

With strikers without visible screws and the consistent locking rail, ECO SLIDE CO combines maximum functionality with an elegant appearance.

### Image IV: SIE\_PORTAL\_ECO SLIDE CO\_Detail\_Mittelverschluss.jpg

High-quality version: the RC2-compatible centre lock and the strikers, integrated in a locking rail, combine security and design.

|  |  |  |
| --- | --- | --- |
| Publisher  SIEGENIA GROUP  Marketing Communications  Industriestraße 1 - 3  D-57234 Wilnsdorf Germany  Tel.: +49 271 3931-1176  E-mail: pr@siegenia.com  www.siegenia.com | Edited by / Contact  Kemper Kommunikation  Kirsten Kemper  Am Milchbornbach 10  D - 51429 Bergisch Gladbach Tel.: +49 2204 9644808  E-mail: info@kemper-kommunikation.de  www.kemper-kommunikation.de | Text Information  Pages: 2  Words: 482  Characters: 3 117 (with spaces)  Created: 2023-06-06 |
| Please send us a sample copy of any publication containing this text or these images. | | |